## Inventory

1. start with 8 x 16 flexible plate plate

2. place 8x16 base on top of 8x16 plate

3. place 9window cupola one row back from one short end of 8x16 base with open end of cupola facing aft.

4. add 2, 2x4 bricks on iether side of base with an overhang of 2x2 directly behind cupola.

5. add one 2x10 brick lengthwise down the starboard side of 8x16 base.

6. add one 2X8 & 2x2 lengthwise down the port side of base

7. from the aft add a layer of 2x2 bricks on top of the bricks placed in step 6 & 7.

8. place 8x8 grate on top of cupola with forward edge flush with forward edge of cupola.

9. place 8x8 plate on top of 8x8 grate.

10. place 2, 1x4 bricks on forward edge of 8x8 plate.

11. place 2, 1x6 bricks on port and starboard edges of 8x8 plate.

12. place castle tower centered and 2 rows back from front of 8x8 plate.

13. place 2x16 plate centered on aft of 8x16 base with 2x3 overhang

14. place brace on port side as ladder to top 8x8 plate.

15. place mast on aft end of 2x6 plate in previous step

16. place 1x2 tall piece under 2x6 plate overhang from step 14.

17. place 2x4 on forward edge of 2x6 plate.

18. place 2x3 plate on top of castle from step 12.

19. place 2, 2x2 bricks on forward corners of 8x6 base one connection only.